Press Release  Press Release  Press Release  Press Release  Press Release

Address:
1F, No. 6,
Alley 6, Lane 45,
Pao Hsin Road,
Hsin Tien City,
Taipei County, Taiwan, R. O. C 

Tel:886-2-2912-1234 Fax:886-2-2913-0792

Contact:
Mr. James Lee ext. 618

	

SBC-554V
Intel Pentium MMX/AMD K6 PISA-bus CPU Card with on-board LCD controller & Flash Disk

The SBC-554V is a PISA bus CPU card with on-board CRT/LCD controller and the revolutionary new DiskOnChip Flash Disk. With its new PISA bus architecture, it can support both ISA and PISA-bus expansions on a single half-size CPU card.

The on-board C&T 65554 video controller is a high performance LCD/CRT Windows accelerator. It supports a wide range of flat panel displays, including 36-bit TFT panel displays. The DiskOnChip supports system boot-up and memory storage up to 72 MB. The on-board VGA/LCD controller and DiskOnChip Flash Disk let you avoid using precious expansion slots for peripheral devices. In addition, you will not have to buy additional boards, worry about compatibility or deal with other vendors.

The SBC-554V also includes two high speed serial ports (one RS-232, one RS-232/ 422 485), one multi-mode (EPP/EPP/SPP) parallel port, a floppy drive controller, an Ultra DMA/33 enhanced IDE controller and a keyboard/PS/2 mouse interface.

The AAEON single board computer includes everything you need for fast, worry-free industrial PC performance. The SBC-554V includes the following features:

��	Half-size PISA bus CPU card
AAEON has pioneered the development of the PISA (PCI+ISA) bus half-size CPU  card. The SBC-554 supports both ISA and PCI-bus expansion cards.
��	Accepts Intel Pentium P54C, P55C, AMD K5/K6 & Cyrix M1/M2 processors
��	Built-in C&T 65554 CRT/LCD controller supports up to 36-bit TFT panels
��	DiskOnChip (solid state disk) socket supports up to 72 MB Flash disk
��	Bus Master IDE supports Ultra DMA/33